|  |  |  |
| --- | --- | --- |
| Cp-10 |  | SMA cp-10 fault troubleshooting 0103 |

***Notes: First response is always to verify current grid conditions.***

1. **Visual References:**



## Figure 1

## *Fault Descriptions and Likely Causes:*

SMA: Grid over voltage slow.

This indicates voltage exceeded inverter high limits.

1. Nearby grid equipment operating
2. Storms or lightning
3. Possibly associated with a subsequent inverter failure
4. ***Troubleshooting***
5. ***Reference material***
6. Text

[Insert picture]

Figure 2 – text

[insert picture]

Figure 3 – text

[insert picture]

Figure 4 – text

1. Text
2. ***Part information***